**List of Finishes**

* Gravel bedding for laying of tiles
* Internal floor 60\*60 gress tiles
* Gypsum Plastering through out the apartment
* Waterproofing in balconies
* External Ceramic Tiles (for balconies)
* Balcony Railings
* Main door
* Marble/ granite Window Sills
* PVC Double Glazing Apertures
* All External Walls on the façade will be covered with insulated Polystyrene and Plastered with GR 1000 and finish of Silicati

**Common Parts**

* Marble/granite Stairs
* Aluminum Railings
* Passenger Lift
* Plastering with two Coats of White Paint
* Letter Boxes
* Wooden Main door
* Water & Electricity Meter Cabinets
* Waterproofing for the Roof of the Block
* PVC Double Glazing Apertures

Water and electrical meters of apartments and common parts are not included